{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["技术要求","腹腔镜镜头","VIVID E95彩超探头技术参数要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"merged":[[0,0,0,5],[5,0,5,1],[5,2,5,5],[6,0,7,5]],"flags":["formulas_cached_only"]}
["采购项目清单：超声探头、腹腔镜镜头等医疗设备配件采购项目"]
["标段","项目名称","数量或规模","资金预算（万元）","资金来源","备注"]
["1标段","GE VIVID E95彩超探头",1,11,"自筹"]
["2标段","腹腔镜镜头",2,13.7,"自筹"]
["合计",null,3,24.7]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：  超声探头、腹腔镜镜头等医疗设备配件采购项目  \n二、项目用途说明：                          \n三、配置规格、附件及零配件（包括专用工具）： \n                                                                                                     \n四、详细技术要求、参数及产品资料等：\n  附技术偏离表、评分标准、产品彩页、相关证明文件      \n                                            \n                                                            \n五、售后服务条件及交货日期（或工期）：\n                                                                                                         \n五、推荐供应商清单\n    一、除公开招标、单一来源外的其他院内采购方式，可推荐三家以上供应商，并且要具有可比性。\n    二、填写内容包括供应商名称、联系人、联系方式，产地、品牌或资质。\n推荐供应商1                                                \n                                                         \n推荐供应商2                                                \n                                                         \n推荐供应商3                                                \n                                                         \n推荐供应商4                                                \n                                                         \n推荐供应商5                                      "]

{"sheet":"腹腔镜镜头","index":1,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,5,0]],"flags":["formulas_cached_only"]}
["腹腔镜镜头\n\n1、单孔30°腹腔镜。\n2、直径5.5㎜，长度50CM，中心分辨率≥20lp/mm。\n3、30°柱状晶体镜，直径5.5毫米，超广角，激光焊接、蓝宝石镜片防划通透，防雾。\n3、可浸泡、气薰、高温高压消毒。\n4、STORZ宫腹一体机专用\n5、质保期≥1年"]

{"sheet":"VIVID E95彩超探头技术参数要求","index":2,"n_rows":12,"n_cols":3,"rows_kept":12,"flags":["formulas_cached_only"]}
["序号","项目","技术参数"]
[1,"探头类型","线阵探头，用于各种小器官：甲状腺、乳腺、男性外生殖系统等以及全身肌肉、肌腱、血管、神经、骨膜等浅表组织检查."]
[2,"标称频率","6.0MHz"]
[3,"B摸式频率范围","3.0-10.0MHz"]
[4,"探测深度","≥120mm"]
[5,"侧向分辨率","≤1mm"]
[6,"轴向分辨率","≤1mm"]
[7,"盲区","≤2mm"]
[8,"横向几何精度","≤5%"]
[9,"纵向几何精度","≤5%"]
[10,"切片厚度","≤7mm"]
[11,"质保期","壹年，质保期内出现质量问题免费更换，并提供备用探头"]