{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","工程量清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":6,"rows_kept":6,"merged":[[0,0,0,5],[4,0,4,1],[4,2,4,5],[5,0,5,5]],"flags":["formulas_cached_only"]}
["采购项目清单：康复分院北楼改造项目"]
["序号","项目名称","数量或规模","资金预算（万元）","资金来源","备注"]
[1,"康复分院北楼改造项目",null,33.43,"自筹"]
["合计"]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量： 康复分院北楼改造 \n二、项目用途说明：                \n三、配置规格、附件及零配件（包括专用工具）： \n1、详情见后附工程量清单。2、工期为20天。                                   \n                                                       \n四、详细技术要求、参数及产品资料等：\n①、税务登记证、营业执照、组织机构代码或三证合一的营业执照。②、法人签字并加盖公章的委托书。③、被委托人的身份证。④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）。⑤、“近三年内参加招投标活动在经营活动中没有重大违法违纪记录”的书面声明。⑥、须具有贰级以上（含贰级）（且符合资质证书承揽范围）装饰装修资质，具有合格有效的企业安全生产许可证；拟派项目经理应具有二级或二级以上建筑工程专业注册建造师资格，且具备有效的安全生产考核合格证书。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。                                         \n五、售后服务条件及交货日期（或工期）：\n①、质量承诺（包括质保期）；②、响应院方工期要求，若承诺的工期不能按时完成，按合同约定进行处罚；③、安全承诺：施工中做好施工组织，保证安全生产，防止人为的对场区管网的损坏。如有安全事故或对场区管网损坏，其造成的伤害事故及一切经济损失，由施工企业承担全责；④、合同外增项按原招标优惠比率结算。                                               \n\n五、推荐供应商清单\n一、除公开招标、单一来源外的其他院内采购方式，可推荐三家以上供应商，并且要具有可比性。\n二、填写内容包括供应商名称、联系人、联系方式，产地、品牌或资质。\n推荐供应商1                                              "]

{"sheet":"工程量清单","index":1,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,7,4]],"flags":["formulas_cached_only"]}
["康复分院北楼改造工程量清单\n1、墙面刷外墙漆面积：\n西侧和东侧：（11.6x14)x2面+(10.5x14)x2面=471.8㎡\n南侧和北侧:(33.5x14)x2面=938㎡\n合计1409.8㎡\n东楼:(19.8x14)x2=554.4㎡\n东楼西侧造型面:103㎡\n小计：2067.2㎡\n2、室内安装成品装饰木门：（含门套，五金）：0.9x2.6x75套=175.5㎡\n室内安装成品双开木门：（含门套，五金）：1.8x2.6x7套=32.76㎡\n3、电器安装：（仅限国内一线品牌）\n2.5mm²铜芯线(两芯)：3000m\n4mm²铜芯线(两芯)：1500m\n6mm²铜芯线(两芯)：1500m\n10mm²铜芯线(两芯)：1500m\n网线4800m\n电话线2400m\n塑料线盒：1000m\nLED节能照明灯具：89个\n消防应急灯：12个\n消防疏散指示灯：15个\n消防监控摄像头：10个"]